BusinessPhone Communication Platform 4.0
Dialogs

## Call Pick-Up Group Parameters

The Group dialog shows all group members of a call pick-up group. A group member is identified by its extension number. A call pick-up group may have up to 20 members. It is also possible to assign one extension to several call pick-up groups.

To access the dialog, open the “Groups” menu in the Configuration directory tree and click on “Call Pickup”. In the Call Pickup Code dialog, click on the Parameters link of a directory number. The Call Pickup Groups dialog is displayed. Click on the Parameters link of a group to open the Call Pick-Up Group Parameters dialog.

For more information about the call pick-up group parameters, see also command 4201 Group members.

### Assigning a new member to a call pick-up group

- In the Group dialog, enter the new member’s extension number in one of the fields (0-19). For example, if the new group should have six members, enter the directory number of each extension in the fields 0 to 5.
- Click on the Submit button.

Note

If the entered extension number does not exist or causes a conflict with an existing directory number, an error message will appear. Read the error message carefully to solve the problem.

- The dialog refreshes, now showing the extension number of the new group member in the respective field.
- Now you can assign other group members or return to the previous dialog by clicking on the Back button.

### Changing or deleting a call-pick up member:

- In the Group dialog, mark the extension number of the group member you want to remove from the call pick-up group.
- Enter the number of a new member or delete the extension number if you do not want to add a new member.
- Click on the Submit button.

Note

If the entered extension number does not exist or causes a conflict with an existing directory number, an error message will appear. Read the error message carefully to solve the problem.

- The dialog refreshes, now showing the changes in the respective field.
- Now you can edit other group members or return to the previous dialog by clicking on the Back button.

#### Actions

Submit |  | To send the settings to the system. |
Reload |  | To load the current system settings and to discard all entered data or changes. |
Back |  | To return to the previous dialog. |

For more information about the call pick-up feature in general, see facility descriptions:

- Call pickup - extension group (143/15534-ASB 150 02 Uen).
- Call Pick-Up – Common (142/15534-ASB 150 02 Uen).

Revision: A © Ericsson Enterprise 2003