BusinessPhone Communication Platform 4.0
Commands > Commands 3000...3999

## 3028
Day/night trunk group 6

This command is used to state which A-categories are permitted to alter the function for day/night switching with respect to trunk group 6. The procedure for day/night switching = *86#

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003