BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x32
No Process For Message

Default definition: |  | ERROR + TRIG |
Used by block: |  | ALL |
Category: |  | DESIGNER |

A message is received to a nonexistent process.

- D1:
- D2: Received INFCODE
- D3: Received SUBCODE
- D4: Received DATA+1

If ‘OS.WARNING code,DY’ is not used, data D3 and D4 are supplied by OS from the ME-register.

Revision: F © Ericsson Enterprise 2003