BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8402
Predigit for carrier access

This command defines the predigits of trunks which can be accessed via the programmed internal access code (8401 Internal access code)

See command 1015 Pre-digits for number analysis, Predigits for number analysis

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003