BusinessPhone Communication Platform 4.0
Fault Tracing ASB 150 02 > Procedures

## Update of board positions

Read the revision states of the hardware positions, RASC-menu MAINTENANCE-HW/SW-RP.

Highlight the relevant row with the cursor and update the board. All programmable data is assigned default values. For extensions and trunks it is also necessary to assign all individuals a telephone number. Normally it should be possible to load configuration data from RASC provided back-up exists.

Revision: F © Ericsson Enterprise 2003