BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8602
Announce directory number ?

When a guest extension is diverted to the individual mailbox system, a welcome announcement is played. In this command it is stated if the directory number of the called extension shall be played or not. If the directory number shall be included (yes), the voice prompt welcome 1 + directory number + welcome 2, storing is played (see commands 8601 Guest extension welcome 1 during storing a message and 8603 Guest extension welcome 2 during storing a message for the voice prompts). If the directory number is not to be included (no), only welcome 1, storing is played.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003