BusinessPhone Communication Platform 4.0
Dialogs

## ASB 150 02 licensing

### License Status

The license status table provides read only information for following values:

- Licensing board
  States the board position which carries the license file
- Remaining trial time
  States the remaining operating hours for all features which have no valid entry in the license file. Licensed features are indicated in the Licensed feature table with a value in the “Release” and “#” column. The counter will be decreased in 5 minutes steps.
- System ID
  States either the serial number of the connected FECU or the serial number the CPU-D5. If a CPU-D5 is installed in the system with a connected FECU, then always the FECU serial number will be used as the system ID.
- Serial Number of Flash Disk
  States the unique serial number of the storage media on which the license file is stored.

### ’Licensed feature’ table

The table provides an overview of all features which are requiring a license

- Feature Name
  States all the features (feature packages) which require a license entry.
- Release
  States the dedicated system release of the licensed feature (prepared for future purpose).
- #
  States the licensed number of the users or the feature level of the license feature

If a listed feature does not contain an entry in the “Release” and “#” column then this feature is not licensed or does not have a valid entry in the license file. In this specific case the feature is active until the “Remaining trail time” elapses.

Values in the ’Licensed feature’ table:

Feature Name | Value (#) | Description
BASIC_LICENSE | 1 | initial value
MOBILE_EXT_LICENSE | 5 -100 | 5 -100 users (in steps of five)
UNIFIED_MSG_LICENSE | 20 -200 | 20 -200 users (in steps of five)
CTI_LICENSE | 5 | 5 users
80 | 80 users
NETWORKING | 3 | Standard digital networking with unlimited trunk interfaces
4 | Full digital networking with 32 trunk interfaces
5 | Full digital networking with unlimited trunk interfaces
VOIP_GATEWAY | 1 | initial value

Note

The Unified Messaging license entry requires in addition also a CTI license entry.
(£ 20 Unified Messaging users 5 CTI users are required, >20 Unified Messaging users, 80 CTI users are required).

Note

The software VoIP Gateway license requires also the corresponding VoIP Gateway IPU license (see IPU - Software licensing).

Note

The VoIP Gateway license entry disables all other license entries.

#### Actions:

- Export license file
  This button is used to fetch the license file from the board on which it is stored and to export it to a desired destination on the PC or LAN. For further details see To export the license file.
- Import license file
  This button is used to import a license file, which was received from the Ericsson License Center, into the system to replace the existing one. For further details see To import the license file
- Show license file
  This button is used to view the content of the license file. For further details see Show license file.
- Reload
  This button is used to refresh all indications from the license dialog.

For further details please refer to: ASB 150 02 R14 (and higher) Software licensing

Revision: A © Ericsson Enterprise 2003