BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8450
Cost time scheme special

This command is used to define the cost level for the carrier, depending on time and day type. Up to 4 (32-35) special cost time schemes can be defined. Each cost time scheme can have 16 (0-15) different cost levels.

The cost level refers to the cost level in the definition table of the pulse cost level or in the definition table of the duration cost level, where it is used to calculate the cost of a fictive call.

Cost time scheme no: |  | 32-35 |
Relative cost level: |  | 0-15 |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003