BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0301
Key function

This menu shows the function of the progammable keys for the selected extension.

This command states which function a key is to have.

For some key functions it is possible to program an associated number, how incoming calls are to be presented and ACD-group priority. See also commands 0302 Number/ID, 0303 Ringing alternative and 0304 ACD-group priority.

If an extension is programmed as a guest extension, command 0118 Guest extension ?, or as a data extension, key 0 is used as wake-up key and data line respectively. It is then not possible to alter the function of key 0.

Note however that these functions cannot be entered with command 0301 Key function.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003