BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x09
No Available Individual At TSU

Default definition: |  | ERROR |
Default limit: |  | 100 |
Used by block: |  | TS |
Category: |  | DESIGNER |

All individuals for the current type of tone at TSU are busy.

- D1: Type of tone, repetitive or non-repetitive
- D2: Current state
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003