BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1107
Busy voice announcement at day

For external incoming calls which are routed to the trunk answering or rerouting position, a voice announcement can be supplied in case of a busy position. This command is used to state the day reference number for this voice announcement.

Valid values for the reference number are:

00-63 (view command 4424 Announcements for trunks) blank (no voice announcement)

The stated reference must have been recorded previously on a system telephone in accordance with command 4424 Announcements for trunks.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003