BusinessPhone Communication Platform 4.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## D3 IPSIG

RP IP signalling

01h IPSETUP |  | Setup to/from H.323 client |
02h IPSETUPACK |  | RP Setup Acknowledge to/from H.323 client |
03h IPPROCEED |  | Call proceeding to H.323 client |
04h IPALERTING |  | Alerting to/from H.323 client |
05h IPCONNECT |  | Connect to/from H.323 client |
06h IPRELEASE |  | Release to/from H.323 client |
07h IPCONP |  | Connected party info to H.323 client |
08h IPCWAIT |  | Call waiting indication |
09h IPCLIP |  | Calling party display info |
0Ah IPINQUIRY |  | Inquiry from H.323 client |
21h IPREGISTER |  | .323 client has registered |
22h IPUNREGISTER |  | H.323 client has unregistered |

.

Revision: PD2 © Ericsson Enterprise 2003