BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0179
TCD suffix dialling-day COS

The command states to which trunk number category for suffix dialling during register recall to PSTN the extension belongs to when the exchange is day-switched. The trunk number category controls which numbers the extension can dial. see command 0103 TCD-day COS for more information.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003