BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x83
EK-Error

Default definition: |  | ERROR + TRIG |
Used by block: |  | EX |
Category: |  | DESIGNER |

The current EK-state was not compared correctly to the current process / instrument state, e.g. there is no free EK, but the instrument state was indicating that all EK’s should be free.

- D1:
- D2: Current process / instrument state.
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003