BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2101
Recall on parking

An extension parking a call for common pickup will be recalled after a predetermined time, if no other extension picks up the call.

This command defines the period of time after which the parking extension will be recalled.

0 = |  | No recall

1- 255 = |  | Recall time in seconds

An external call that is parked for common pickup will be diverted to the external line’s diversion position after approx. 11 minutes if not being picked up before.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003