BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0151
Tenant group

The command defines which tenant group the extension belongs to in a multi PABX application.

In detail this means that if several customers share one ASB 150 they can separate their extensions into a maximum of 16 tenants.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003