BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1930
Pre-digit removal for private plan with unknown type of number

This command specifies the number of pre-digits to be removed to get the internal number for “called party” for an incoming ISDN-call using number plan private, and the number type is UNKNOWN.

Value: 00-15

Country specific settings

The following parameters should be programmed. For the other parameters the default value is to remain.

Country | UN | LOC | NAT | INT | NET
Australia | - | X | X | - | -
Austria | - | - | - | - | -
Belgium | - | X | X | - | -
Italy | - | X | X | - | -
Netherlands | - | X | X | - | -
Sweden | - | - | - | - | -
Spain | - | - | - | - | -
Finland | - | X | X | - | -
Denmark | X | - | X | - | -
New Zealand | - | X | X | - | -

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003