BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2057
Follow me/Diversion to ACD

The command defines whether follow me, direct diversion or diversion on busy to an active ACD group is allowed-on default the command is deactivated, that means follow me, direct diversion respective diversion on busy is not allowed.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003