BusinessPhone Communication Platform 4.0
Commands > Commands 5000...5999

## 5532
Delete Private Network Access

In ASB 150 02, the private network router (PNR) is intended to be an own isolated routing mechanism, which will have the following main tasks:

- Routing based on dialled private network access code
- 3 alternative route selections in case of busy trunks
- Destination number conversion based on choosen route

This command will delete a private network access code (PNAC) with the stated directory number.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003