BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x1F
Map Placement Error, Not Activated

Default definition: |  | ALARM + NOPROG + EXTERN + ACTIVE |
Used by block: |  | OS |
Category: |  | MAINTENANCE |

A program map is not placed in the expected position. The map will not be activated.

- D1: Expected position, read from the map header.
- D2: Actual position.
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003