BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0xA3
SP Program Memory Error

Default definition: |  | ALARM + NOPROG + EXTERN + ACTIVE |
Used by block: |  | SP |
Category: |  | MAINTENANCE |

The serial communication processor (SP) on the CPU board has found a program memory checksum error.

- D1:
- D2:
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003