BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0118
Guest extension ?

In hotels the extensions are divided into guest extensions and service extensions.

This command states whether the extension shall be a guest extension (Y) or a service extension (N).

As a rule guest extensions are assigned special telephones. They have access to facilities such as wake-up and do not disturb, but not to facilities such as follow-me and information.

For guest extensions the PICKUP-key is used for the wake-up function. Consequently, for guest extensions, command 0301 Key function cannot be used to alter the function of the PICKUP-key.

For other hotel commands see command group 80.

It is not possible for an extension to be both a guest extension and a data extension at the same time.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003