BusinessPhone Communication Platform 4.0
Dialogs

## Subscription

This dialog is used to handle the Cordless telephones.

Note

You cannot add any extension numbers in this dialog. This is done automatically, using the existing BMS data.

The directory numbers of Card/Individual addresses are mapped to line connections. In this dialog, you can handle Master/Slave assignments as well. The description complies to the directory name of the BMS data.

If you need to subscribe a new extension, an additional window will open. Here you can enter an IPEI code. After submission, the PARK and Access Code are sent back.

You must synchronize the DECT data, if the directory number and/or the primary/secondary assignment of a cordless extension has been changed. You will also receive a warning message, if BMS detects any deviations. Additionally, a SYNC button will appear to solve this problem.

In case of an inconsistency due to an other application that modified the data partially, the same functionality will be available.

The dialog displays the following data:

- Number (of the primary telephone and the own number, if the Cordless is used as a secondary telephone)
- Directory name
- Address
- BMS board position (Card/Individual)
- Status

#### Actions

Subscribe/Unsubscribe |  | The lettering of the button depends on the status of the Cordless extension. |

Revision: A © Ericsson Enterprise 2003