BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8426
Discount factor metering

This command is used only if calculation is based on duration.

This command defines for the tenant and the selected carrier the extent the cost specified in the DURATION COST LEVEL DEFINITION TABLE should be modified (in %) before it is used to calculate the call cost.

Range of pulse cost LCR: 10 digits plus decimal point

Minimum required authority level from telephone:

Accessible via BMS:

Revision: A © Ericsson Enterprise 2003