BusinessPhone Communication Platform 5.1
Commands > Commands 5000...5999

## 5505
Delete group call pick up code

In ASB 150 a pickup group is formed from a list of extensions. In case of a call to a member of the group another member can answer the call from his/her own telephone by dialling the code for “group call pickup”.

With this command the group call pickup facility can be deleted.

Deletion of the call pickup code also leads to deletion of all call pickup groups.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: C © Ericsson Enterprise 2003