BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4321
Maximum number of active OCN users

This command states how many users may have active notification at the same time. If this limit is reached then no more users are allowed to activate notification.

In 4320 Notification scheduling profile - the maximum number of user in dependence of

- min. allowed trunks and
- min. scheduling profile,

are described.

Revision: PD1 © Ericsson Enterprise 2003