BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## C8 CILDIGSEND

0 CLDIG |  | Digits transmitted to external destination |
1 CLACCINIT |  | (Re)start reception of Account Code digits |
2 CLACCDIG |  | Account Code digits |
3 CLLCRDIAL |  | Dialled digits at LCR-analyzed calls |
4 CLLCRSENT |  | Sent digits at LCR-analyzed calls |
5 CLPNRSENT |  | Sent digits at private network router |
6 CLACCREQ |  | Request for Account Code digits |
7 CLACCACK |  | Sending of Account Code |
8 CLACCNAK |  | No Account Code |
0 CLVLDSND |  | Validity data |
1 CLVLDCON |  |  |

Revision: PD2 © Ericsson Enterprise 2003