BusinessPhone Communication Platform 5.1
Dialogs

## Extension Parameter

The Extension Parameter dialog is the main dialog for the extension management. This dialog comprises all settings and details that you can configure for an extension.

To access the parameter dialog of an extension, open the “Extensions” menu in the Configuration directory tree and click on one of the submenus (Analog, Cordless, or Digital). Alternatively, you can select the context menu of the Extensions main menu as well. The context menu appears. Select “List extensions” to open the extension list dialog. Now click on a directory number to bring up the Extension Parameter dialog.

On top of the parameter dialog, you find a navigation bar showing the different sections of the dialog:

- General
- Assignment
- Active Features
- Passive Features
- Diversion
- Loudspeaker Paging
- Programmable keys
- Individual Short Numbers

Use the navigation bar to go to each section.

### Selecting commands and extensions

To select a parameter, mark the respective check box in the first column of a table. All parameters that you have checked are included if you want to copy the extension data to another extension later on.

On top of the dialog, you will find a check box called “(Un)Select all commands”. This is a toggle box: If no command has been checked, you can select all commands with just one click. If all commands in the list are checked, click in the check box to deselect all commands.

To view and edit the parameters of an extension, select a number from the Directory Number drop-down list box. Alternatively, you can enter the directory number directly in the field aside and click on the “Go to extension” link.

For more information about a setting or a field, click on the command link in brackets to open the online help system.

See also facility description General (15534-ASB 150 02 Uen).

### Commands

Note

The displayed data depends on the extension type, the extension assignment, the system connection mode and on the system version. Additionally, the dialog may look different in offline and online mode.

#### General

5601 |  | Extension directory number

6501 |  | Directory name

#### Assignment

0101 |  | Facility COS

0103 |  | TCD-day COS

0104 |  | TCD-night COS

0105 |  | Common abbreviated number COS

0179 |  | TCD suffix dialling-day COS

0180 |  | TCD suffix dialling-night COS

0151 |  | Tenant group

0102 |  | Traffic group

0174 |  | Alarm group

5630 |  | Assigned slave

0118 |  | Guest extension?

0191 |  | Call cabin extension?

0125 |  | Voice mail extension?

0175 |  | Use as CTI operator instrument?

0145 |  | Relay control

#### Active Features

0146 |  | Meter info allowed on display?

0148 |  | Automatic display of metering info?

0147 |  | Type of meter info

0165 |  | Diversion on no reply to slave?

0166 |  | Slave always logged on?

0167 |  | Ring on master and slave?

0160 |  | Password check at message retrieving?

0501 |  | Access to common mailbox?

0189 |  | Conversation recording allowed?

0177 |  | Initiate callback in corporate network?

0170 |  | Number/name secrecy to corporate network?

0176 |  | Call diversion to corporate network allowed?

0182 |  | Network intrusion?

0171 |  | Travelling class mark

0116 |  | Destination

0144 |  | Delay time

0152 |  | Override LCR?

0153 |  | Direct carrier access LCR?

0154 |  | Limit routing choices LCR

0149 |  | Number secrecy to public network?

0178 |  | ISDN caller list allowed?

0169 |  | Directory number subscribed in PSTN?

0150 |  | Individual charging?

0188 |  | Voice transmission quality

0190 |  | Switch to non-IP network allowed?

0117 |  | Authority code

0163 |  | RTR from extension enabled?

0155 |  | Disable call state message to line?

0186 |  | Handle cordless display texts?

0183 |  | Access to directory book allowed?

#### Passive Features

0106 |  | Call back allowed?

0108 |  | Camp-on allowed?

0107 |  | Break-in allowed?

0161 |  | Music channel in hold state?

0164 |  | DDI to extension enabled?

0181 |  | Permanent immediate answer allowed?

0114 |  | Ringing line 1

0115 |  | Ringing line 2

0121 |  | DTMF to instrument?

0122 |  | Long ring bursts?

0124 |  | Call waiting tone for analogue extensions?

0187 |  | Expensive route warning tone?

#### Diversion

0112 |  | Destination

0109 |  | Diversion active?

0159 |  | Direct diversion?

0110 |  | Diversion on no reply?

0111 |  | Diversion on busy?

0156 |  | Direct diversion?

0157 |  | Diversion on no reply

0158 |  | Diversion on busy?

0119 |  | Diversion time long

0120 |  | Diversion time short

0123 |  | Repeated call diversion?

0184 |  | Individual external diversion at internal calls

0185 |  | Individual external diversion at external calls

0172 |  | Destination for internal calls

0173 |  | Destination for external calls

#### Loudspeaker Paging

4801 |  | Member of loudspeaker paging group 0

4802 |  | Member of loudspeaker paging group 1

4803 |  | Member of loudspeaker paging group 2

4804 |  | Member of loudspeaker paging group 3

4805 |  | Member of loudspeaker paging group 4

4806 |  | Member of loudspeaker paging group 5

4807 |  | Member of loudspeaker paging group 6

4808 |  | Member of loudspeaker paging group 7

4809 |  | Loudspeaker paging volume

#### Actions

Submit |  | To set the changed parameters. |
Reload |  | To reload the current parameters from the PBX (if connected). |
Copy |  | To load a dialog for copying parameters to other extensions. |
Back |  | To return to the previous window. |

Revision: B © Ericsson Enterprise 2003