BusinessPhone Communication Platform 5.1
Dialogs

## Private Network Router

The facility creation dialog is used to create and delete facilities, change their directory numbers and names and select a facility for parameter editing.

To access the dialog, open the “Facilities” menu in the Configuration directory tree. Then open the “Networking” submenu and click on “Private Network Router”.

If no private network router has been created before, only the following command is available:

5432 |  | Create Private Network Access Code

### Creating a facility

To create a new facility, enter the directory number in the “Directory Number” field in the “Create Private Network Router” section and click on the Create button.

If you have changed any directory numbers or directory names you will be asked whether you want to discard your changes. If you want to save your changes first, click on Cancel and press the Submit button before creating the new group.

See also section Private Network Router - Copy Settings.

### Changing a directory number and/or directory name

To change a Directory Number or Name, edit the numbers or names displayed in the Edit/Change Group section and click on the Submit button.

### Editing the facility parameters

Most facilities have parameters that can be changed. To view and edit these parameters, click on the Parameters link of the desired facility. If a directory number/name has been changed, you will be asked whether you want do discard these changes. To save your changes, choose Cancel and submit your changes before you click on the Parameters link.

See dialog description Private Network Router -Parameters.

### Deleting a facility

To delete a facility, click on the facility’s Delete link. BMS will display a delete dialog. See section Private Network Router Delete.

See Facility Descriptions:

- Networking – Based On Analogue Lines
  (361/15534-ASB 150 02 Uen).
- Networking – VPN Service From PSTN
  (364/15534-ASB 150 02 Uen).
- Networking – Based On Digital Lines
  (365/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003