BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6602
Administrative data for extensions and trunk lines

This command group consists of commands for the handling of administrative data records for defined extensions and trunk lines.

These commands are used to create, alter or delete a data record. The data record is assigned to a directory number. The directory number must be a defined extension or trunk line number. A maximum of 250 records can be stored in the PABX. Use command 6501 Directory name, if the directory number is not defined in the PABX.

Note

that it is possible to read data records of all extensions, also extension classified as guest telephones.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003