BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3401
Assigning members to a group

The directory numbers that are members of the group need to be programmed.

Initially there are no members.

In case of the selection of parallel distribution via BMS, the programming of members via command 3401 is not possible from an instrument - only scrolling through the list is allowed to do.

Valid values: Extension directory number

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003