BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x75
Invalid Data In RP-Message

Default definition: |  | ERROR |
Used by block: |  | RP |
Category: |  | DESIGNER |

Some data in a message was not accepted by the RP program.

- D1: Offset in the message

- 00h: DATA
- 01h: DATA+1
- etc.

- D2: Received INFCODE
- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003