BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4450
Loading voice announcement

With this command it is possible to load prerecorded announcements from a VMU-HD/MFU board which uses a hard/flash PROM as a strorage memory. If these announcements are already recorded an another board, the references of these announcements first have to be erased with the command 4401 - 4438.

Otherwise loading from the VMU-HD or MFU board is not allowed.

The following list shows the announcements which will be loaded.

command | Character | discription
4401 | 1-32 | General announcements
4402 | 1-7 | Predefined information texts
4403 | 1-12 | Months (language 1)
4404 | 1-31 | Dates (language 1)
4405 | 0-23 | Hours (language 1)
4406 | 0-11 | 5 minutes (language 1)
4407 | 0-23 | Hours (language 2)
4408 | 0-11 | 5 minutes (language 2)
4409 | 0-23 | Hours (language 3)
4410 | 0-11 | 5 minutes (language 3)
4411 | 1-42 | Automated Attendant prompts
4412 | 0-14 | Voice prompts for mailbox system (language 1)
4413 | 0-6 | Voice prompts for mailbox system (language 2)
4414 | 0-6 | Voice prompts for mailbox system (language 3)
4415 | 0-31 | Welcome prompts for storing, individual mailbox
4416 | 0-15 | Welcome prompts for retrieving, individual mailbox
4417 | 0-15 | Welcome prompts for storing, common mailbox
4418 | 0-15 | Welcome prompts for retrieving, common mailbox
4419 | 0-9 | Digits (language 1)
4420 | 0-9 | Digits (language 2)
4421 | 0-9 | Digits (language 3)
4422 | 0-15 | Common system prompts
4423 | 0-10 | DISA voice prompts
4424 | 0-63 | Trunk exit position
4425 | 1-255 | ACD greeting announcements
4426 | 1-24 | CTI - Automated Attendant (AA) voice prompts
4427 | 0-15 | Music on Hold prompts
4428 | 0-25 | Additional mailbox voice prompts
4429 | 1-12 | Months (language 2)
4430 | 1-31 | Dates (language 2)
4431 | 1-12 | Months (language 3)
4432 | 1-31 | Dates (language 3)
4433 | 0-18 | Mailbox content information prompts (language 1)
4434 | 0-18 | Mailbox content information prompts (language 2)
4435 | 0-18 | Mailbox content information prompts (language 3)
4436 | 0-15 | Queue announcements for PBX groups
4437 | 0-13 | Mailbox forward a message + send a message
4438 | 0-21 | Mailbox system - outcall notification

Minimum required authority level from telephone: 1

Accessible via BMS: No

Revision: PD1 © Ericsson Enterprise 2003