BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1917
MCID activation request allowed

The command is used to define whether the Malicious Call Identification facility is subscribed or not for the current ISDN-link from network operator.

The command states whether any MCID facility request is allowed to be sent to the network. This is the case if the facility is subscribed.

The following MCID facility parameters are available:

NO: MCID facility is not subscribed

YES: MCID facility is subscribed

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003