BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8714
Waiting for full directory number

Each AA (its selections list) can be programmed to wait for a complete extension number or for single-digit directory number.

Default value:

NO = if you want that procedure waits for single-digit directory number.

Press Enter to go to the next command.

Note

If selections list has been programmed to wait for a full directory number commands 8703 Digit 0 related dir no-8712 Digit 9 related dir no will be invalid.

Valid values: YES / NO

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003