BusinessPhone Communication Platform 5.1
Commands > Commands 5000...5999

## 5401
Create a route

In ASB 150 a route is a list of trunk lines. When calling the route’s directory number, a free trunk will be seized in accordance with a defined allocation principle.

This command will create a new route with the stated directory number. The route may be given a random directory number, if there is one which does not conflict with existing directory numbers. (See command group 56).

ASB 150 allows a maximum of 255 routes.

Command 3301 Random Selection determines which rule (principle) is to be used for selection of a trunk. Command 3201 Route members defines which trunks are to be included in the route.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: C © Ericsson Enterprise 2003