BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1928
Pre-digit removal for E.164 number plan with network specific typ of number

This command specifies the number of pre-digits to be removed to get the internal number for “called party” for an incoming ISDN-call using number plan E.164, and the number type is NETWORK SPECIFIC.

Value: 00-15

Minimum required authority level from telephone:

Accessible via BMS:

Revision: PD1 © Ericsson Enterprise 2003