BusinessPhone Communication Platform 5.1
Dialogs

## Standard Cost Calculation

You can define the internal access code, the carrier for Least Cost Routing and the actual price of one meter pulse. For more information about this feature, please see the help description of the following commands:

8401 |  | Internal access code

8420 |  | Carrier open

8424 |  | Multiplication factors

To access the Standard Cost Calculation dialog, open the “Features” menu in the Configuration directory tree. Then open the “Call Metering” submenu and click on “Cost Calculation”. The Cost Calculation dialog appears. To access the Standard Cost Calculation dialog, click on one of the Create Carrier links in the Standard Cost Calculation section.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |
Back |  | To return to the Cost Calculation dialog without any changes. |

See facility description Call Metering (141/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003