BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8508
Common mailbox welcome 2

In this command the reference number for the welcome message upon diversion of a hotel extension to a common mailbox is stated. The guest is checked in with the language according to language 2. To program a language code see commands 8009 Wake-up language 1-8011 Wake-up language 3. For each common mailbox a welcome announcement can be programmed.

The welcome announcement is played in the language the guest is checked in with.

The welcome announcement stated in command 8507 Common mailbox welcome 1 is played for a guest extension with language 2, or if the language is unknown. In commands 8508 Common mailbox welcome 2 and 8509 Common mailbox welcome 3 the welcome announcements for language 2 and language 3, respectively, are stated.

The given reference is supposed to have been recorded according to command 4417 Welcome common. Note that recording according to command 4417 is only possible on a VMU-HD board.

Valid values: 0-15

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003