BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2503
Abbreviated number category 1

This command defines whether or not the abbreviated number shall be available for the abbreviated number category 1.

Y = Open for category |  |

N = Blocked for category (default data) |  |

An existing abbreviated number is erased by pressing the “-” -key on the phone. This key can also be used as backspace during programming of an abbreviated number.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003