BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3027
Day/night trunk group 5

This command is used to state which A-categories are permitted to alter the function for day/night switching with respect to trunk group 5. The procedure for day/night switching = *85#

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003