BusinessPhone Communication Platform 5.1
Dialogs

## Fictive Number - List numbers

In this dialog, you can determine the tenants that are allowed to use the number series and assign a diversion address and name to each fictive number. Furthermore, you can hide a fictive number from the common directory.

To access the dialog, open the “Number series” menu in the Configuration directory tree, click on “Fictive” and then click on a series’ directory number link. Alternatively, select the “List numbers” option from the context menu of a number series.

The dialog consists of two parts. The first part shows the directory number, the list length and the authorized tenants that may use the number series.

The second part below shows all fictive numbers, their diversion addresses and assigned names. If you want to mask a fictive number from the directory book, place a tick the “Hidden” check box.

Note

If the list length is 1, 10 or 100, you can view the data on one single page. If the length is 1000, the data is displayed in steps of 100. Use the Previous and Next buttons of the quick navigation bar to browse the pages.

The following commands are available in the dialog:

2830 to 2346 |  | Open for Tenant (0-15)

2530 |  | Diversion address

6501 |  | Assigned name

#### Actions

Submit |  | To submit your changes to the system. |
Next |  | This button is available if the length of a series is 1000. Click on the button to view the next 100 entries. |
Previous |  | This button is available if the length of a series is 1000. Click on the button to view the previous 100 entries. |

See facility description Fictive Number (201/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003