BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x47
Invalid A-Directory Number

Default definition: |  | ERROR |
Used by block: |  | ALL |
Category: |  | DESIGNER |

The callers public directory number (a-directory number) was considered invalid.

- D1:
- D2: Type of directory number

- 00h: Invalid public number group.
- 01h: Invalid caller directory number.
- 02h: DIR.NONUM has been given as input data and no public number digits are programmed (no number to be returned) or a general error.

- D3: Undefined
- D4: Undefined

#### Recommended action

Check the programming of the exchange directory number. Check the programming of the callers directory number.

Revision: PH2 © Ericsson Enterprise 2003