BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3094
Conversation recording

This command defines which A-categories are allowed to record an ongoing conversation. With this command it is possible to enable or disable the access of the initiating party to conversation recording facility for the given ACOS.

The command defines if an extension is allowed to record conversations. If this command is set to NO for a specific extension, it is not possible to initiate conversation recording for this extension.

Note

Please be aware of the legal situation when using the conversation recording feature:
Recording a conversation without prior notice to the other party may be an illegal act. Forwarding or playback of this recorded conversation to a third party without prior permission may be an illegal act.

Valid data: Yes/No

Default data: No
Per default all ACOS values are set to NO, which means that the conversation recording feature is disabled for the whole ASB 150 02 system.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003