BusinessPhone Communication Platform 5.1
Dialogs

## Public Directory Numbers

In this dialog public numbers and types for 32 groups can be specified. You can set the own country code that is used as a prefix for a calling/connected number that is part of a number plan E.164. the prefix is added before the number is sent to the private network.

To access the dialog, open the “System” menu in the Configuration directory tree. Then open the “Number analysis” submenu and click on “Public directory no.”.

The following commands are available:

2236 |  | Own country code

2237 |  | Own area code

2220 |  | Public number

2224 |  | Type

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

See Facility Descriptions:

- Networking – Based On Digital Lines (365/15534-ASB 150 02 Uen).
- Directory Numbers (163/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003