BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2650
Expensive route warning tone

This tone is defined to inform the user about an alternatively choosen route in the PNR for the ongoing call setup.

##### Default data: ( need not to be modified )

Ton Element | Tone Fragment | Signal Time | Pause Time | Repetition Start point
Number | Int. | Ext. | (ms) | (ms) |
1 | 2 | 2 | 320 | 10 | >>..<<
2 |  |  |  |  |
3 |  |  |  |  |
4 |  |  |  |  |

Revision: E © Ericsson Enterprise 2003