BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8011
Wake-up language 3

For wake-up of a guest and for answering wake-up calls, wake-up messages in the form of voice messages can be supplied to the guest.

The wake-up message can be given in three different languages.

With commands 8009 Wake-up language 1-8011 Wake-up language 3 the three languages in which wake-up messages can be given are stated.

The four leading capital characters of the language should be entered, e.g. ENGL for English or SPAN for Spanish.

Commands 8012 Wake-up answer anno 1-8014 Wake-up answer anno 3 and 8015 Wake-up order ref 1-8017 Wake-up order ref 3 are used to determine the wake-up messages to be supplied for the respective language.

When a guest checks in, a language can be stated for the guest. If any of the languages stated with commands 8009 Wake-up language 1-8011 Wake-up language 3 matches the language stated for the guest, the wake-up message will be supplied in that language. Otherwise the wake-up message will be supplied in the 1st language, i.e. the language stated with command 8009 Wake-up language 1.

Valid values: A-Z (initial value=blank)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003