BusinessPhone Communication Platform 5.1
Dialogs

## Dumpfiles - File Manager

This dialog lists all files that have been created using the dump feature of the BMS maintenance part. The dump files are stored in the dump directory of the server. In addition, you can use the dialog to export the system log and the restart data.

To access the dialog, open the “Maintenance” menu in the Configuration directory tree and click on the “Dumpfiles” submenu.

### Downloading a dump file

- Click on the link of the file that you would like to download.
- The Windows Download Manager opens.
- Click in the second button to save the file on your local disk.
- Click on OK.
- Select a directory or create a new directory and click on the Save button. If the saving process is finished, you will see a confirmation.
- Click on the Close button to close the window and to return to the Dumpfiles - File Manager dialog.

### Dumping a system log

- Click on the System Logs button. A new dialog is displayed.
- Enter a file name.
- Check the optional box “Append?” if you want to add the log to a previously saved file.
- Click on the Dump button. The dialog refreshes, now showing the file name in the list. Now you can download or delete the file.

### Dumping restart data

- Click on the Restart Data button. A new dialog is displayed.
- Enter a file name.
- Check the optional box “Append?” if you want to add the log to a previously saved file.
- Click on the Dump button. The dialog refreshes, now showing the file name in the list. Now you can download or delete the file.

### Deleting a dump file

- To delete a dump file, click on the Delete button of the respective file.

#### Actions:

System logs |  | To save the following data to a file: HW details, CPU-SW LZY info, lines, warnings, restart history files, Service Logbook. |
Restart Data |  | To save the following data to a file: CPU-memory map 0 Add. D200 to D6FF Rp-memory card 00 Add. 0020 0000 to 0020 1FFF Rp-memory card 00 Add. 0076 0000 to 0076 FFFF Rp-memory card 00 Add. 0077 0000 to 0077 FFFF |

Revision: B © Ericsson Enterprise 2003