BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6801
Tenant name

This command can be used to define a name for a tenant group. This means that, if several customers share one ASB 150, they can separate their extensions and trunks into a maximum of 16 tenants. A maximum length of 40 characters may be defined as tenant name.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003