BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2273
Automatic Redial Trunk Access Retries

This command defines the number of retries, if no one is free in that moment, that will be executed when automatic redial wants to access a trunk

Every retry will be done in fixed time intervals of 60 seconds.

##### Valid data:

Valid values: |  | 1 - 10 |
Initial values (default): |  | 5 |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003